**[Summary]** [MY22/Multi User/Dev-Signed] Call alert will appear on the PIN UI when reciving an incomming call before unlock the system after ingition cycle (manual 10/10)

**[Precondition]**

**Testing Type:** Eco-mate

**Connected Devices:** Samsung A51 via bluetooth

1. Current user profile is locked by PIN.  
2. A BT device is connected.

**[Test Steps]**

1. Make an ignition cycle and check the BT connection state.  
2. Make an incoming call to the connected BT device.  
3. Unlock the PIN and check the system behavior.

**[Expected Result]**

1. PIN UI shall be shown and BT shall be connected.  
2. BT incoming call alert shall be shown only on phone side.  
3. BT incoming call alert shall be shown in Notification bar

**[Actual Result]**

When receiving incomming call, the call alert can be shown on the PIN locking UI before unlock the PIN after ignition cycle

**[Reproduced Rate]**

10/10

**[Spec Reference]**

N/A

**[Occurrence Time]** ~1/27/2021 16:51:25

**[Comments]**

This issue can’t be reproduced on the previous signed build QIH22B-244\_Devsigned  
  
This issue can reproduce on both dev-sign and user build

**[Hardware Info]**

**CSM:** GB MY22 CSM3.7 PV01H, High, NA

**[Found by running test case]**

TC\_PINUIN\_IgnitionCycle\_027

TC\_PINUIN\_IgnitionCycle\_028

**SW build info:** W99E-W157.3.2-QIH22B-250\_Devsigned

**Contact Phone Number:** +886 966603203

**Submitter:** <<<rick.weng@cienet.com>>